Pre-season commissioning checklist
Checklist. Tick each item or write what you found in Notes. Add your own boat's items at the end of each section.
	Particulars
	

	Fleet number and yacht name
	

	Make and model
	

	Base
	

	First booking of the season
	

	Engine and generator hours
	

	Checked by
	



1. Hull and underwater gear
Do it on the hard if you can. Southern Right Yachting, a yacht manager, says shaft seals, cutless bearings and propellers are best inspected during a haul-out.
	Check
	OK
	Notes

	Hull for damage, blisters and osmosis
	
	

	Antifouling and anodes
	
	

	Through-hulls and seacocks, operated and checked for corrosion
	
	

	Shaft seal, cutless bearing and propeller
	
	

	Keel and rudder, from groundings reported last season
	
	

	Hatches and portlights, checked for leaks
	
	

	
	
	

	
	
	



2. Rig and sails
Southern Right lists the standing and running rigging for chafe and corrosion at the terminals, and the sails for UV damage and blown stitching.
	Check
	OK
	Notes

	Standing rigging, terminals and chainplates
	
	

	Running rigging for chafe
	
	

	Sails, UV strips and stitching
	
	

	Furlers and blocks lubricated and tested under load
	
	

	Winches serviced
	
	

	
	
	

	
	
	



3. Engine and generator
Southern Right's list: oil and filters, coolant, impeller, belts, fuel system, exhaust, and a full test under load. Generators and thrusters are tested too.
	Check
	OK
	Notes

	Oil and filter changed, or hours checked against the schedule
	
	

	Coolant level
	
	

	Raw water impeller inspected or replaced
	
	

	Belts
	
	

	Fuel filters and fuel system
	
	

	Exhaust system
	
	

	Full test under load
	
	

	Generator, thrusters and watermaker tested
	
	

	
	
	

	
	
	



4. Systems
Watermakers, air conditioning, bilge pumps and electrical panels all need testing and servicing where intervals are due, per Southern Right. Batteries should be load-tested and shore power connections inspected.
	Check
	OK
	Notes

	Bilge pumps and float switches
	
	

	Batteries load-tested
	
	

	Shore power inlet and cable for corrosion and wear
	
	

	Electrical panel and breakers
	
	

	Heads, holding tanks and fresh water system
	
	

	Gas system checked and hoses in date
	
	

	Electronics and autopilot
	
	

	
	
	

	
	
	



5. Safety equipment
Life rafts, EPIRBs, flares and fire extinguishers all have service intervals and expiry dates, as Southern Right points out. Check every one lasts the season.
	Check
	OK
	Notes

	Life raft service date
	
	

	EPIRB battery and registration
	
	

	Flares expiry
	
	

	Fire extinguishers serviced
	
	

	Life jackets, harnesses and jackstays
	
	

	First aid kit
	
	

	
	
	

	
	
	



6. Papers for commercial use
A boat in commercial charter needs its paperwork in order. Southern Right names a valid commercial endorsement or licence, a coded or classed safety certificate and up-to-date stability documents.
	Check
	OK
	Notes

	Commercial licence or endorsement
	
	

	Safety certificate or coding certificate, in date
	
	

	Periodic inspection, in countries that require one
	
	

	Insurance for charter use
	
	

	Registration
	
	

	
	
	

	
	
	



7. Work still open
List anything not finished, with the date it will be. A boat with open safety items doesn't take a booking.
	Item
	Safety item?
	Due by
	Signed off
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