Rig survey report
Template. The grey text explains each section: replace it with your own. Delete the example findings before issuing.
	Particulars
	

	Vessel name
	

	Make and model
	

	HIN
	

	Year built
	

	Length overall
	

	Client
	

	Date of survey
	

	Place of survey
	

	Surveyor
	

	Report number
	



1. Particulars
The boat and its rig. The age of the standing rigging is the first thing an insurer asks, so record it and say where the date came from.
Survey: client, date, place, mast stepped or unstepped, report number
Vessel: name, make and model, HIN, year built
Rig: type (masthead or fractional sloop, cutter, ketch), mast and boom maker, number of spreaders, keel- or deck-stepped
Standing rigging: wire or rod, terminals, date fitted and the evidence for it
Furling: headsail and mainsail furlers, make and model
Example: Masthead sloop, Selden two-spreader keel-stepped mast. 1x19 stainless wire with swaged terminals, fitted May 2015 according to the rigger's invoice.

2. Scope of survey
Where you inspected the rig from. A survey from deck level and one with the surveyor aloft find different things, and the reader needs to know which this was.
Whether the mast was stepped or unstepped, and whether you went aloft
Method, such as visual inspection, magnification, dye penetrant on terminals and operating the furlers
Areas you couldn't reach or see, such as the inside of the mast or the masthead sheave
Example: The rig was inspected with the mast stepped. The surveyor went aloft by bosun's chair and inspected all fittings to the masthead. Dye penetrant was used on the lower terminals of the cap shrouds and forestay.

3. Summary of recommendations
Every recommendation once, grouped by grade. Rig failures put people in danger, so A items should say clearly not to sail until they're done.
A, safety: fix before the vessel next sails
B, 12 months: fix within about a year
C, routine: maintenance and notes

4. Mast, spars and fittings
The findings on the mast, boom and spreaders, from the mast step to the masthead, and on the standing and running rigging. Work from the bottom up, or the top down, and keep to one order.
Mast step or deck step, partners and mast foot, with corrosion and compression
Mast tube, sail track, welds and fittings, spreaders and their roots and tips
Masthead, sheaves, crane and instruments
Standing rigging, terminals, toggles, turnbuckles, pins and split pins
Chainplates, their deck seals and their attachment below deck
Furlers, halyards, sheets and blocks
Boom, gooseneck, kicker and mainsheet attachment
	No.
	System
	Location
	Observation
	Recommendation
	Grade

	1
	Standing rigging
	Starboard cap shroud, lower swaged terminal
	Hairline crack along the swage, confirmed with dye penetrant.
	Replace the shroud before the vessel next sails.
	A

	2
	Standing rigging
	Forestay toggle at the stemhead
	Clevis pin held by a split pin with only one leg opened, and no tape.
	Fit a new split pin, opened correctly, and tape it.
	A

	3
	Chainplates
	Port aft lower shroud chainplate, at the deck
	Sealant failed, with rust staining on the deck and a damp bulkhead below.
	Remove the chainplate, inspect it for crevice corrosion, replace if pitted and rebed. Check the bulkhead for rot.
	B

	4
	Mast
	Mast foot on the keel step
	White corrosion powder and pitting where the aluminium heel sits on the steel step.
	Unstep at the next haul-out, clean, treat and isolate the heel from the step.
	B

	5
	Spreaders
	Upper spreader tips, both sides
	Spreader boots split, and the wire shows wear where it bears on the tip.
	Renew the boots and check the wire for broken strands.
	B

	6
	Furler
	Headsail furler, drum
	Drum turns stiffly and the bearing is noisy.
	Service the furler bearings to the maker's instructions.
	C



	Grade
	Meaning

	A: Safety
	Safety or compliance deficiency. Fix before the vessel is next underway.

	B: 12 months
	Deficiency that needs timely attention. Fix within about 12 months.

	C: Routine
	Note or observation, cosmetic or maintenance. Routine maintenance at the owner's convenience.



5. Rig age and replacement
Your view on the age of the standing rigging and when to replace it. Many insurers ask about rigging older than 10 to 15 years, and some limit cover for it.
The age of the standing rigging and the evidence for it
How the boat has been sailed, if known, such as offshore or coastal
Your recommendation on replacement, with a date
Example: The standing rigging is 11 years old. No defects were found in the wire, but insurers commonly ask for replacement at this age, and crevice corrosion inside swaged terminals can't be seen. Replacement is recommended before the 2027 season.

6. Conclusion
Whether the rig is fit for use, on what conditions, and for what kind of sailing.
The overall condition of the rig
Whether it is fit to sail once the A items are done, and any limits

7. Surveyor's certification
Your statement, name, qualifications and signature.
Statement of independence and who may rely on the report
Name, qualifications and membership number
Signature and date of issue
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