Tender survey report
Template. The grey text explains each section: replace it with your own. Delete the example findings before issuing.
	Particulars
	

	Vessel name
	

	Make and model
	

	HIN
	

	Year built
	

	Length overall
	

	Client
	

	Date of survey
	

	Place of survey
	

	Surveyor
	

	Report number
	



1. Particulars
The tender and the yacht it belongs to. Tenders change hands with the yacht, and insurers list them separately, so record the builder's plate in full.
Survey: client, parent yacht, date, place, report number
Tender: make and model, HIN, year built, length, hull material, tube material (Hypalon, PVC or polyurethane)
Builder's plate: design category, maximum persons, maximum load and maximum engine power
Propulsion: outboard, inboard or jet, with make, model, serial number, power and hours
Example: 4.2 m RIB, built 2021, GRP hull, Hypalon tubes. Builder's plate: design category C, 6 persons, maximum engine power 60 hp. Outboard 50 hp, 380 hours.

2. Scope of survey
What you inspected and how. Say whether the tender was ashore, in the water or in its garage on the yacht, and whether you ran it.
Where the tender was inspected and whether it was launched
Method, such as visual inspection, a pressure hold test on the tubes and a run in the water
What wasn't inspected, such as tube areas hidden by fendering or the hull under the chocks

3. Summary of recommendations
Every recommendation once, grouped by grade.
A, safety: fix before the tender is next used
B, 12 months: fix within about a year
C, routine: maintenance and notes

4. Inspection findings
The findings, from the tubes to the engine. Tube and seam failures and corroded lifting points cause most tender losses and injuries, so give them the most attention.
Tubes, seams, valves, rubbing strakes and handles, with the pressure hold result
Hull, keel, transom and its bond to the tubes
Outboard or inboard, steering, controls and kill cord
Fuel tank, lines and venting
Lifting points and their bonding to the hull, for a crane or davit
Battery, wiring, navigation lights and bilge pump
	No.
	System
	Location
	Observation
	Recommendation
	Grade

	1
	Lifting points
	Aft port lifting eye, inside the transom
	Backing plate corroded, with rust staining in the laminate around the fastenings.
	Remove the lifting eye, inspect the fastenings and backing plate, and replace them. Do not lift the tender by crane until done.
	A

	2
	Tubes
	Starboard tube, aft chamber
	Lost 40 percent of its pressure in 12 hours on the hold test. Bubbles at the valve seat when tested with soapy water.
	Replace the valve and repeat the pressure hold test.
	A

	3
	Propulsion
	Kill cord, helm console
	Kill cord missing. The engine starts without it.
	Fit a kill cord and check it stops the engine.
	A

	4
	Tubes
	Bow, both tubes, at the rubbing strake
	Hypalon coating worn through to the base fabric over 10 cm from contact with the yacht's garage door.
	Patch the worn area and fit a protective strip.
	B

	5
	Hull
	Hull underside, keel line
	Scratches from beaching. No damage to the laminate.
	No action needed. Note for the next survey.
	C



	Grade
	Meaning

	A: Safety
	Safety or compliance deficiency. Fix before the vessel is next underway.

	B: 12 months
	Deficiency that needs timely attention. Fix within about 12 months.

	C: Routine
	Note or observation, cosmetic or maintenance. Routine maintenance at the owner's convenience.



5. Safety equipment
The gear the tender should carry for its use, with expiry dates.
Lifejackets for the maximum number of persons
Kill cord, paddles or oars, bailer or pump, anchor and line
Fire extinguisher on an inboard or a tender with a fixed fuel tank
Flares and a handheld VHF if the tender goes beyond sight of the yacht

6. Conclusion
The overall condition and whether the tender is fit for use once the A items are done.

7. Surveyor's certification
Your statement, name, accreditation and signature.
Statement of independence and who may rely on the report
Name, accreditation and membership number
Signature and date of issue
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